I/0 RECOVERY by Graham Pollock
Appeared in Australian MiCo October 1985 P41
----------------------------------------------------------
File: BASIC

Have you ever Spent 3 hours typing in a  program only to find that you CSAVED the first copy on the leader and your other 2 copies have got I/0 ERRORS right smack in the middle of them.  What do you do?  You SCREAM of course.

No more screaming! Here's a utility which will come to your rescue.  After you RUN it, you can CLOAD your bad tape and recover, MOST of  your   program.  Notice that  I said  "most" and "not all". You will have to go through the program and add the bit or bits which have been left out.  While the tape is CLOADing you are told each time an error has occurred. This will only react  to an I/O ERROR  and mico behaves in a normal way for FM and OM ERRORS.

