MC-10 Operation and Language Reference Manual Appendix E

Appendix E/Specifications
AC Power Adapter (required) |
Catalog Number | 26-3011
Power Input | 120V AC 60Hz 16W
Power Output | 8.0V AC 1.5A AC
Microprocessor |
Type | 6803
Physical Dimensions |
Size | 2" (H) x 8 1/2" (L) x 7" (W) (51mm x 216mm x 178mm)
Weight | 29 1/2 ozs. (836.32 grams)
Temperature |
Operating | 41 degrees to 104 degrees (Fahrenheit) 5 degrees to 40 degrees (Centigrade)
Storage | -40 degrees to 160 degrees -40 degrees to 71 degrees
Humidity |
Operating | 40% to 80%
Storage | 20% to 90%
Serial Interface
RS-232-C Signal | Pin #
CD Carrier Detect | 1
RD Receive Data | 2
GND Ground | 3
TD Transmit Data | 4
Printer Software Requirements 600 baud 1 Start Bit 7 Data Bits 2 Stop Bits No parity 132-Column printer width Automatic Carriage return at end of line Cassette Interface Suggested Input Level for Playback from Recorder 1 to 5 V peak-to-peak at a minimum impedance of 220 ohms Typical Computer Output Level to Recorder 800 mV peak-to-peak at 1K ohms Remote Ground Signal Ground Remote Control Input from Recorder's EARphone Jack Output to Recorder's AUX or MIC Jack

Comments should be directed to the following email address:
dsbrain@neosplice.com